//****************************************************************************
//                            INTEL CONFIDENTIAL
//                     Copyright 2009 - 2011 Intel Corporation
//                           All Rights Reserved.
// 
// The source code contained or described herein and all documents related to
// the source code ("Material") are owned by Intel Corporation or its
// suppliers or licensors. Title to the Material remains with Intel
// Corporation or its suppliers and licensors. The Material contains trade
// secrets and proprietary and confidential information of Intel or its
// suppliers and licensors. The Material is protected by worldwide copyright
// and trade secret laws and treaty provisions. No part of the Material may be
// used, copied, reproduced, modified, published, uploaded, posted,
// transmitted, distributed, or disclosed in any way without Intel's prior
// express written permission.
// 
// No license under any patent, copyright, trade secret or other intellectual
// property right is granted to or conferred upon you by disclosure or
// delivery of the Materials, either expressly, by implication, inducement,
// estoppel or otherwise. Any license under such intellectual property rights
// must be express and approved by Intel in writing.
// 
//****************************************************************************
//
//  Date:  February 18, 2009
//  Description:  Field Replaceable Unit (FRU) data file for the Intel Server
//  Board S5500WB.
//
//****************************************************************************


_LF_NAME       'WB_BMC.fru'  // Name for this load file
_LF_VERSION    '0.05'        // Version of this load file
_LF_FMT_VER    '1.50'        // Version of the load file format
_IPMI_VERSION  '1.00'        // IPMI format version

_FRU (
_FRU_TITLE     'Baseboard FRU' // FRU Title
_START_ADDR    0000        // Start Address
_DATA_LEN      0130        // Data Length
_NVS_TYPE      'IMBDEVICE' // Non-volatile Storage Type
_DEV_BUS       FF          // Device Bus
_DEV_ADDRESS   20          // Device Address

_SEE_COMMON						// 8 bytes
   01                 // Common Header Format Version
   01                 // Internal Use Area Starting Offset (in multiples of 8 bytes)
   02                 // Chassis Info Area Starting Offset (in multiples of 8 bytes)
   10                 // Board Info Area Starting Offset (in multiples of 8 bytes)
   19                 // Product Info Area Starting Offset (in multiples of 8 bytes)
   00                 // MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                 // Pad
   D3                 // Common Header Checksum

_SEE_INTERNAL					// 8 bytes
   01                 // Internal Use Format Version
   00
   00
   00
   00
   00
   00
   03

_SEE_CHASSIS          // 0x6A bytes
   01                 // Chassis Info Area Format Version Bit Fields
   0E                 // Chassis Info Area Length (in multiples of 8 bytes)
   17                 // Chassis Type (Main Server Chassis)
   D2                 // Chassis Part Number, 0x12 bytes
   '..................'
   D2                 // Chassis Serial Number, 0x12 bytes
   '..................'
   DF                 // Custom Chassis Info type/length byte for AM1 (For Microsoft WHQL use), 0x1F bytes
   '...............................'
   DF                 // Custom Chassis Info type/length byte for AM2 (For OEM use), 0x1F bytes
   '...............................'
   C1                 // End of field marker

_SEE_BOARD						// 0x46 bytes
   01                 // Board Info Area Format Version Bit Fields
   09                 // Board Info Area Length (in multiples of 8 bytes)
   00                 // Language Code
   000000             // Mfg. Date/Time
   D1                 // Board Manufacturer, 0x11 bytes
   'Intel Corporation'
   C7                 // Board Product Name, 0x07 bytes
   'S5500WB'
   CC                 // Board Serial Number, 0x0C bytes
   '............'
   CA                 // Board Part Number (Contains the PBA#), 0x0A bytes
   '..........'
   CC                 // FRU File version ID string, 0x0C bytes
   'FRU Ver 0.05'
   C1                 // End of field marker


_SEE_PRODUCT					// 0x5F bytes
   01                 // Product Info Area Format Version Bit Fields
   0D                 // Product Info Area Length (in multiples of 8 bytes)
   00                 // Language Code
   D1                 // Product Manufacturer Name, 0x11 bytes
   'Intel Corporation'
   C7                 // Product Name, 0x07 bytes
   'S5500WB'
   CA                 // Product Part Number (Contains the Top Assembly (TA)#), 0x0A bytes
   '..........'
   D4                 // Product Version (Available for OEM use), 0x14 bytes
   '....................'
   CC                 // Product Serial Number, 0x0C bytes
   '............'
   D4                 // Asset Tag (Available for OEM use), 0x14 bytes
   '....................'
   C0                 // FRU File ID (Not used)
   C1                 // End of field marker



)
